CPVC



Submittal Information

CPVC Saddle Blast Gate

|  |
| --- |
| * Constructed from CPVC Sheet and are Used

 in Ventilation Systems* Welded Construction using 5/32”C PVC Welding

Rod* All Dimensions in Inches
* All Dimensions are to CSSI Standards and are

Subject to change. |
|  |
|  |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

CPVC SADDLE BLAST GATES SUBMITTAL INFORMATION

Model Number Nominal Duct Size OD Pipe Size A B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SBG-CPVC-4 | 4 | 4.5 + 1/16 | 11.9687 | 7.75 |
| SBG-CPVC-6 | 6 | 6.625 + 1/16 | 14.0625 | 9.5 |
| SBG-CPVC-8 | 8 | 8.625 + 1/16 | 17.125 | 11.5 |
| SBG-CPVC-10 | 10 | 10.75 + 1/16 | 20.25 | 14 |
| SBG-CPVC-12 | 12 | 12.75 + 1/16 | 23.3125 | 16 |
| SBG-CPVC-14 | 14 | 14 + 1/16 | 26.375 | 17 |
| SBG-CPVC-16 | 16 | 16 + 1/16 | 29.25 | 19 |
| SBG-CPVC-18 | 18 | 18 + 1/16 | 32.3125 | 21.25 |
| SBG-CPVC-20 | 20 | 20 + 1/16 | 35.375 | 23.25 |
| SBG-CPVC-24 | 24 | 24 + 1/16 | 38.25 | 27.25 |