

Submittal Information

PVC End Caps

F

* Standard Size End Caps Fabricated From Seamless

Extruded PVC Duct

* End Caps Are Triple-Pass Welded Using 5/32” PVC

Welding Rod

\*Depending on Size, End Caps May Have 1-2 Seams

* All Dimensions are in Inches
* All Dimensions are to CSSI Standards and are Subject to Change

PRODUCT DIMENSIONS

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | |  | |  | |  | |  | | |  | | |  | | --- | | **ALL DIMENSIONS ARE TO CSSI STANDARDS AND ARE SUBJECT TO CHANGE** | |  |  | | --- | |  | |

PVC END CAPS SUBMITTAL INFORMATION

Model Number Nominal Duct Size Average Duct O.D. Average Wall Thickness A Length

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA-PVC-6 | 6 | 6.625 | 0.187 | 6.625 + 1/16 | 3.25 | |
| CA-PVC-7 | 7 | 7.375 | 0.187 | 7.375 + 1/16 | 3.25 |
| CA-PVC-8 | 8 | 8.625 | 0.187 | 8.625 + 1/16 | 3.25 | |
| CA-PVC-9 | 9 | 9.375 | 0.187 | 9.375 + 1/16 | 3.25 | |
| CA-PVC-10 | 10 | 10.75 | 0.187 | 10.75 + 1/16 | 3.25 | |
| CA-PVC-12 | 12 | 12.75 | 0.187 | 12.75 + 1/16 | 3.25 | |
| CA-PVC-14 | 14 | 14 | 0.187 | 14 + 1/16 | 3.25 | |
| CA-PVC-16 | 16 | 16 | 0.187 | 16 + 1/16 | 3.25 | |
| CA-PVC-18 | 18 | 18 | 0.187 | 18 + 1/16 | 3.25 | |
| CA-PVC-20 | 20 | 20 | 0.219 | 20 + 1/16 | 3.25 | |
| CA-PVC-24 | 24 | 24 | 0.25 | 24 + 1/16 | 3.25 | |