Submittal Information



PVC 45 Degree Wye Saddle

F

|  |
| --- |
| * Constructed from PVC Duct For Use In   Ventilation Systems   * Fitting Pieces Triple-Pass Welded Using 5/32”   PVC Welding Rod   * All Dimensions in Inches |
|  |
| * All Dimensions are to CSSI standards and are   Subject to Change |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

PVC 45 DEGREE WYE SADDLE DIMENSIONS CHART

SOCKET

Model Number Nominal Size A B “B” End Type

|  |  |  |  |
| --- | --- | --- | --- |
| SA45-PVC-6-6 | 6 ON 6 | 6.625 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-7 | 6 ON 7 | 7.375 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-8 | 6 ON 8 | 8.625 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-9 | 6 ON 9 | 9.375 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-10 | 6 ON 10 | 10.75 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-12 | 6 ON 12 | 12.75 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-14 | 6 ON 14 | 14 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-16 | 6 ON 16 | 16 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-18 | 6 ON 18 | 18 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-20 | 6 ON 20 | 20 + 1/16 | 6.625 + 1/16 |
| SA45-PVC-6-24 | 6 ON 24 | 24 + 1/16 | 6.625 + 1/16 |
|  |  |  |  |
|  |  |  |  |
| SA45-PVC-7-7 | 7 ON 7 | 7.375 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-8 | 7 ON 8 | 8.625 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-9 | 7 ON 9 | 9.375 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-10 | 7 ON 10 | 10.75 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-12 | 7 ON 12 | 12.75 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-14 | 7 ON 14 | 14 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-16 | 7 ON 16 | 16 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-18 | 7 ON 18 | 18 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-20 | 7 ON 20 | 20 + 1/16 | 7.375 + 1/16 |
| SA45-PVC-7-24 | 7 ON 24 | 24 + 1/16 | 7.375 + 1/16 |