CPVC



CPVC Blast Gate

Submittal Information

|  |
| --- |
| * Constructed from CPVC Duct and Type I PVC Sheet   For Use in Ventilation Systems   * Welded Construction using 5/32” CPVC Welding   Rod   * All Dimensions in Inches * All Dimensions are to CSSI Standards and are   Subject to change. |
|  |
|  |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

CPVC BLAST GATE SUBMITTAL INFORMATION

Model Number Nominal Duct Size A B\* C\* Fully Opened Gate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| BG-CPVC-3 | 3 | 3.5 + 1/16 | 7.75 | 11 | 15.25 |
| BG-CPVC-4 | 4 | 4.5 + 1/16 | 7.75 | 11 | 15.25 |
| BG-CPVC-6 | 6 | 6.625 + 1/16 | 9.75 | 13.75 | 20 |
| BG-CPVC-7 | 7 | 7.375 + 1/16 | 10.75 | 15 | 22 |
| BG-CPVC-8 | 8 | 8.625 + 1/16 | 11.75 | 16 | 24.25 |
| BG-CPVC-9 | 9 | 9.375 + 1/16 | 12.75 | 17 | 26 |
| BG-CPVC-10 | 10 | 10.75 + 1/16 | 14.25 | 20 | 30.375 |
| BG-CPVC-12 | 12 | 12.75 + 1/16 | 16.25 | 22 | 34.375 |
| BG-CPVC-14 | 14 | 14 + 1/16 | 17.25 | 24 | 37.625 |
| BG-CPVC-16 | 16 | 16 + 1/16 | 19.25 | 27 | 42.625 |
| BG-CPVC-18 | 18 | 18 + 1/16 | 21.5 | 30 | 47.625 |
| BG-CPVC-20 | 20 | 20 + 1/16 | 23.5 | 33 | 52.562 |
| BG-CPVC-24 | 24 | 24 + 1/16 | 27.5 | 39 | 62.5 |

\*Within ¼”

