CPVC



Submittal Information

CPVC Gravity Damper

|  |
| --- |
| * Constructed from CPVC Duct and Type I PVC Sheet   For use in Ventilation Systems   * Welded Construction using 5/32” CPVC Welding   Rod   * All Dimensions in Inches * All Dimensions are to CSSI Standards and are   Subject to change. |
|  |
|  |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

CPVC GRAVITY DAMPER SUBMITTAL INFORMATION

Model Number Nominal Duct Size A\* B\* C\* Bolt Hole

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| GD-CPVC-4 | 4 | 6 | 5 | 9 | 1/2 |
| GD-CPVC-6 | 6 | 7.625 | 6.625 | 11 | 1/2 |
| GD-CPVC-8 | 8 | 9.625 | 8.625 | 13.50 | 1/2 |
| GD-CPVC-9 | 9 | 10.375 | 9.375 | 15 | 1/2 |
| GD-CPVC-10 | 10 | 11.750 | 10.750 | 16 | 1/2 |
| GD-CPVC-12 | 12 | 13.750 | 12.750 | 19 | 1/2 |
| GD-CPVC-14 | 14 | 15 | 14 | 21 | 1/2 |
| GD-CPVC-16 | 16 | 17 | 16 | 23.50 | 1/2 |
| GD-CPVC-18 | 18 | 19 | 18 | 25 | 1/2 |
| GD-CPVC-20 | 20 | 21 | 20 | 27.5 | 1/2 |
| GD-CPVC-24 | 24 | 25 | 24 | 32 | 1/2 |

