CPVC



Submittal Information

PVC Saddle Blast Gate

|  |
| --- |
| * Constructed from PVC Sheet and are Used   in Ventilation Systems   * Welded Construction using 5/32” PVC Welding   Rod   * All Dimensions in Inches * All Dimensions are to CSSI Standards and are   Subject to change. |
|  |
|  |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

PVC SADDLE BLAST GATES SUBMITTAL INFORMATION

Model Number Nominal Duct Size OD Pipe Size A B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SBG-PVC-4 | 4 | 4.5 + 1/16 | 11.9687 | 7.75 |
| SBG-PVC-6 | 6 | 6.625 + 1/16 | 14.0625 | 9.5 |
| SBG-PVC-8 | 8 | 8.625 + 1/16 | 17.125 | 11.5 |
| SBG-PVC-10 | 10 | 10.75 + 1/16 | 20.25 | 14 |
| SBG-PVC-12 | 12 | 12.75 + 1/16 | 23.3125 | 16 |
| SBG-PVC-14 | 14 | 14 + 1/16 | 26.375 | 17 |
| SBG-PVC-16 | 16 | 16 + 1/16 | 29.25 | 19 |
| SBG-PVC-18 | 18 | 18 + 1/16 | 32.3125 | 21.25 |
| SBG-PVC-20 | 20 | 20 + 1/16 | 35.375 | 23.25 |
| SBG-PVC-24 | 24 | 24 + 1/16 | 38.25 | 27.25 |