CPVC

CPVC Butterfly Damper



Submittal Information

|  |
| --- |
| * Constructed from CPVC Duct and Type I CPVC Sheet   For Use in Ventilation Systems   * Welded Construction using 5/32” CPVC Welding   Rod   * All Dimensions in Inches * All Dimensions are to CSSI Standards and are   Subject to change. |
|  |
|  |

PRODUCT DIMENSIONS

|  |
| --- |
|  |

CPVC BUTTERFLY DAMPER SUBMITTAL INFORMATION

Model Number Nominal Duct Size Connection I.D. A\* B\* C\*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| D-CPVC-6 | 6 | 6.625 + 1/16 | 8 | 12 | 10.5 |
| D-CPVC-7 | 7 | 7.375 + 1/16 | 8 | 12 | 11.3 |
| D-CPVC-8 | 8 | 8.625 + 1/16 | 8 | 12 | 12.5 |
| D-CPVC-9 | 9 | 9.375 + 1/16 | 10 | 14 | 13.2 |
| D-CPVC-10 | 10 | 10.75 + 1/16 | 10 | 14 | 14.6 |
| D-CPVC-12 | 12 | 12.75 + 1/16 | 12 | 16 | 16.6 |
| D-CPVC-14 | 14 | 14 + 1/16 | 14 | 18 | 17.9 |
| D-CPVC-16 | 16 | 16 + 1/16 | 16 | 20 | 20.3 |
| D-CPVC-18 | 18 | 18 + 1/16 | 18 | 22 | 22.3 |
| D-CPVC-20 | 20 | 20 + 1/16 | 20 | 26 | 24.3 |
| D-CPVC-24 | 24 | 24 + 1/16 | 30 | 36 | 28.3 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| \*Within ¼ Inch |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

