Submitatal Information

CPVC Reducer

F



|  |
| --- |
| * Custom Sized Reducers Available Upon Request
* Constructed From I CPVC Sheet for use in

Ventilation Systems* All Dimensions in Inches
 |
|  |
| * All Dimensions are to CSSI standards and are

 Subject to Change |

Note: if height is a concern please contact CSSI

PRODUCT DIMENSIONS

|  |
| --- |
|   |

CPVC REDUCER SPECIFICATION CHART

 SOCKET

Model Number Nominal Reducer Size A B End Type

|  |  |  |  |
| --- | --- | --- | --- |
| RE-CPVC-6-4 | 6 TO 4 | 6.625 + 1/16 | 4.5 + 1/16 |
| RE-CPVC-8-4 | 8 TO 4 | 8.625 + 1/16 | 4.5 + 1/16 |
| RE-CPVC-8-6 | 8 TO 6 | 8.625 + 1/16 | 6.625 + 1/16 |
| RE-CPVC-10-6 | 10 TO 6 | 10.75 + 1/16 | 6.625 + 1/16 |
| RE-CPVC-10-8 | 10 TO 8 | 10.75 + 1/16 | 8.625 + 1/16 |
| RE-CPVC-12-6 | 12 TO 6 | 12.75 + 1/16 | 6.625 + 1/16 |
| RE-CPVC-12-8 | 12 TO 8 | 12.75 + 1/16 | 8.625 + 1/16 |
| RE-CPVC-12-10 | 12 TO 10 | 12.75 + 1/16 | 10.75 + 1/16 |
| RE-CPVC-14-6 | 14 TO 6 | 14 + 1/16 | 6.625 + 1/16 |
| RE-CPVC-14-8 | 14 TO 8 | 14 + 1/16 | 8.625 + 1/16 |
| RE-CPVC-14-10 | 14 TO 10 | 14 + 1/16 | 10.75 + 1/16 |
| RE-CPVC-14-12 | 14 TO 12 | 14 + 1/16 | 12.75 + 1/16 |
| RE-CPVC-16-8 | 16 TO 8 | 16 + 1/16 | 8.625 + 1/16 |
| RE-CPVC-16-10 | 16 TO 10 | 16 + 1/16 | 10.75 + 1/16 |
| RE-CPVC-16-12 | 16 TO 12 | 16 + 1/16 | 12.75 + 1/16 |
| RE-CPVC-16-14 | 16 TO 14 | 16 + 1/16 | 14 + 1/16 |
| RE-CPVC-18-8 | 18 TO 8 | 18 + 1/16 | 8.625 + 1/16 |
| RE-CPVC-18-10 | 18 TO 10 | 18 + 1/16 | 10.75 + 1/16 |
| RE-CPVC-18-12 | 18 TO 12 | 18 + 1/16 | 12.75 + 1/16 |
| RE-CPVC-18-14 | 18 TO 14 | 18 + 1/16 | 14 + 1/16 |
| RE-CPVC-18-16 | 18 TO 16 | 18 + 1/16 | 16 + 1/16 |
| RE-CPVC-20-10 | 20 TO 10 | 20 + 1/16 | 10.75 + 1/16 |
| RE-CPVC-20-12 | 20 TO 12 | 20 + 1/16 | 12.75 + 1/16 |
| RE-CPVC-20-14 | 20 TO 14 | 20 + 1/16 | 14 + 1/16 |
| RE-CPVC-20-16 | 20 TO 16 | 20 + 1/16 | 16 + 1/16 |
| RE-CPVC-20-18 | 20 TO 18 | 20 + 1/16 | 18 + 1/16 |
| RE-CPVC-24-12 | 24 TO 12 | 24 + 1/16 | 12.75 + 1/16 |
| RE-CPVC-24-14 | 24 TO 14 | 24 + 1/16 | 14 + 1/16 |
| RE-CPVC-24-16 | 24 TO 16 | 24 + 1/16 | 16 + 1/16 |
| RE-CPVC-24-18 | 24 TO 18 | 24 + 1/16 | 18 + 1/16 |
| RE-CPVC-24-20 | 24 TO 20 | 24 + 1/16 | 20 + 1/16 |

“B” END TYPE